## Noise Sentry Instrument Driver Readme

To rate this instrument driver, go to the driver download page on the Instrument Driver Network.

#### 1. Overview

Instrument Driver Technology: LabVIEW Plug and Play (project-style)
Manufacturer: Convergence Instruments
Supported Language(s): LabVIEW
Supported Model(s): Noise_Sentry V1.00, V1.10, V1.20, V1.30, V1.40
Model(s) Tested: Noise_Sentry V1.00, V1.10, V1.20 , V1.30, V1.40
Interface(s): USB-Serial
Firmware Revision(s) Tested: V1.00, V1.10, V1.20, V1.30, V1.40
Certified: No
NI Supported: No
Source Code Available: Yes
Driver Revision: 1.4
Original Release Date: 09/17/2009
Current Revision Date: 09/13/2010

#### 2. Required Software

Some software components need to be installed before using this instrument driver. The minimum versions of these components are listed below, and can be downloaded from the Download Site.

LabVIEW 9.0.1 or later
VISA 4.5 or later
Refer to the LabVIEW Help for more information about software requirements. You access the LabVIEW Help by selecting Help»Search the LabVIEW Help.

#### 3. Known Issues

To report issues or provide feedback about this instrument driver, please send an email to instrument.drivers@ni.com.

#### 4. Revision History

The latest version of this and other LabVIEW and LabWindows/CVI instrument drivers can be downloaded at the Instrument Driver Network.
REV 1.0, 09/17/2009

Original release.

REV 1.1, 01/29/2010

- Modified log output format for better clarity.

- Included calibration correction within the read_log VI for consistency with the Noise_Sentry_mk2_Management library

REV 1.2, 05/24/2010

- Added support for firmware revision 1.30

REV 1.3, 05/31/2010

- Added support for firmware revision 1.40

REV 1.4, 09/13/2010

- Modified so that driver could be rebuilt automatically by new versions of LabVIEW

Developed by Bruno Paillard